1. Boulder Retards, Item SPV.0060.xx.
A  Description
This special provision describes furnishing and placing boulder retards in the tributary to the Milwaukee River
B  Materials
Furnish boulder retards with a diameter of 18 to 24 inches, and conforming to the pertinent requirements of standard spec 606.2.  Obtain Wisconsin Department of Natural Resources (DNR) approval of the boulder retards prior to placement.
C  Construction
Place boulder retards conforming to standard spec 606.3.3 and as shown in the plans.
The exact location of the boulder retards will be determined by the DNR.  Coordinate this work with the DNR and notify the DNR a minimum of 7 days prior to boulder placement to allow DNR oversight during boulder placement.  The DNR contact is Kristina Betzold, WDNR, at (414) 343 - 9346.
D  Measurement
The department will measure Boulder Retards as each individual boulder retard acceptably completed. 
E  Payment
The department will pay for the measured quantity at the contract unit price under the following bid item:
ITEM NUMBER	DESCRIPTION	UNIT
SPV.0060.xx	Boulder Retards	EACH
Payment for Boulder Retards is full compensation for furnishing and placed each Boulder Retard.
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