1. Precast Panels for Soldier Pile Walls, Item SPV.0165.xx.
A  Description
This special provision describes fabricating, furnishing, transporting and erecting precast concrete panels for soldier pile walls.
B  Materials
B.1 General
Furnish precast panels that conform to the details shown on the plans.
Furnish steel reinforcement conforming to standard spec 505.
Furnish Grade A air-entrained concrete conforming to standard spec 501.
B.2 Plant Certification
Obtain all precast concrete panels from fabrication plants that comply with the department’s plant certification program in standard spec 106.3.3.3.1.
C  Construction
C.1 General
Prior to fabricating panels, verify that no field modifications were made to the top of footing elevations. Field modifications will require adjustments to the panel heights listed on the plans.
C.2 Placing Concrete
Handle and place the concrete conforming to standard spec 502.3.5.
C.3 Curing
Cure the concrete panels by any of the methods specified in standard spec 502.3.8.
C.4 Transportation, Storage, and Erection
Transport, handle, store, and erect precast panels in a way that prevents cracking or other damage to the panels.  Discard and replace units damaged by improper handling or storing.
D  Measurement
The department will measure Precast Panels for Soldier Pile Walls by the square foot acceptably completed.
E  Payment
The department will pay for the measured quantity at the contract unit price under the following bid item:
ITEM NUMBER	DESCRIPTION	UNIT
SPV.0165.xx	Precast Panels for Soldier Pile Walls	SF
Payment is full compensation for the fabrication, furnishing, transporting, and erecting of precast concrete panels for soldier pile walls.
SPV.0165.xx (20260917)
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