[bookmark: _Hlk23751538]Designer Notes:  This special provision is for contractor-designed temporary support for staged bridge construction.  The engineer of record retains the responsibility to ensure that a contractor-designed temporary support is feasible and practicable, and that the remaining structure is able to handle the staged traffic prior to the advertisement and letting of the project.
1. Temporary Support Enter Structure #, Item SPV.0060.xx.
A  Description
This special provision describes the design, construction, maintenance, and removal of a temporary support system for staged construction of a bridge deck as shown on the contract plans. 
B  Materials
Furnish materials conforming to standard spec part 5: Structures.  
B.1 Design
All dead, live, and construction loading conditions shall be determined by the contractor.
[bookmark: _Hlk126218209]B.2 Plan Requirements and Submittals
Provide plans and submit conforming to standard spec 526.3.3.
C  Construction
Construct the temporary support system conforming to standard spec 526.3.4.
D  Measurement
The department will measure Temporary Support Enter Structure # as each support acceptably completed.
E  Payment
The department will pay for the measured quantity at the contract unit price under the following bid item:
ITEM NUMBER	DESCRIPTION	UNIT
SPV.0060.xx	Temporary Support Enter Stucture #	EACH
Payment for Temporary Support Enter Stucture # is full compensation for designing, constructing, maintaining, and removing the temporary support system as called for in the plans.
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