1. Adjusting Diaphragms, Item SPV.0060.xx.
A  Description
This special provision describes adjusting diaphragms and cross frames where girders are vertically realigned.  Perform the work conforming to standard spec 506.
B  (Vacant)
C  Construction
Remove connections as necessary to reposition the cross frames and diaphragms.  Disassemble the diaphragms and cross frames, clean and prime contact areas of diaphragms, cross frames, stiffeners and connection plates with an approved zinc-rich primer, and reassemble with new ASTM A325 bolts.  
D  Measurement
The department will measure Adjusting Diaphragms by the individual adjusted diaphragm acceptably completed.
E  Payment
The department will pay for the measured quantity at the contract unit price under the following bid item:
ITEM NUMBER	DESCRIPTION	UNIT
SPV.0060.xx	Adjusting Diaphragms	EACH
Payment for Adjusting Diaphragms is full compensation for disassembling, cleaning, priming, reaming, drilling and reassembling diaphragms and cross frames with new ASTM A325 bolts.
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